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[bookmark: _Toc424222693][bookmark: _Toc182825174]Purpose
This document provides Rules and Conditions applicable to ICS2 Information exchange messages. 
[bookmark: _Toc424222695][bookmark: _Toc182825175]Target Audience
[bookmark: _Toc424222696]The intended audience for this document are the representatives of the Member States and trade, any person involved in ICS2 project.
[bookmark: _Toc182825176]Structure of this document
The present document contains the following chapters:
· Chapter 1 – Introduction: describes the scope and the objectives of the document;
· Chapter 2 – Rules : provides a list of rules to be used in ICS2 information exchange messages.
· Chapter 3 – Conditions: provides a list of conditions to be used in ICS2 information exchange messages.
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	Ref.
	Title
	Reference
	Version
	Date

	R01
	
	
	
	

	R02
	
	
	
	

	R03
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	Abbreviation/Acronym
	Definition

	ECCG
	Electronic Customs co-ordination Group

	M
	Mandatory

	O
	Optional

	RIMSCO
	The Risk Management Strategy Implementation Coordination Group
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	R3002
	In the 'ADDRESS' class either 'ADDRESS/Street' and 'ADDRESS/Number' or 'ADDRESS/P.O.Box' has to be used.



	R3003
	This attribute has to be unique as per Declarant (DECLARANT/Identification number) or Person notifying the arrival (Person notifying the arrival/Identification number).



	R3004
	The MRN shall be generated using the following structure:
Last two digits of year of the registration (n2)
Identifier of the country where the message is addressed to (a2)
Unique identifier per year and country (an11)
Trader interface identifier (a1)
Procedure identifier (a1)
Check digit (an1)



	R3005
	EORI number shall be declared.



	R3006
	When 'COMMUNICATION/Type' is 'TE' the 'COMMUNICATION/Identifier' has to have an international phone number format as defined in the ITU-T recommendation E.123 (02/2001). The format must be compliant with the pattern "^\\+(?:[0-9] ?){6,14}[0-9]$”.



	R3007
	Either 'ACTIVE BORDER TRANSPORT MEANS/Conveyance reference number' or 'ACTIVE BORDER TRANSPORT MEANS/Identification number' and 'ACTIVE BORDER TRANSPORT MEANS/Type of identification' must be used.



	R3008
	Either 'CONSIGNMENT (HOUSE LEVEL)/PASSIVE BORDER TRANSPORT MEANS' or 'CONSIGNMENT (HOUSE LEVEL)/GOODS ITEM/PASSIVE BORDER TRANSPORT MEANS' must be used.



	R3009
	When 'ACTIVE BORDER TRANSPORT MEANS/Type of identification' is '10' this attribute must contain IMO ship identification number and its value must be made of the three letters "IMO" followed by a six-digit sequential unique number and a check digit. The check digit is calculated by multiplying each of the first six digits by a factor of 2 to 7 corresponding to their position from right to left. The rightmost digit of this sum is the check digit.



	R3010
	When 'ACTIVE BORDER TRANSPORT MEANS/Type of identification' is '80' this attribute must contain unique European Vessel Identification Number (ENI) and its value must have an eight digit format.



	R3011
	When 'ACTIVE BORDER TRANSPORT MEANS/Mode of transport' is '1' the value of this attribute must be '10'.



	R3012
	When 'ACTIVE BORDER TRANSPORT MEANS/Mode of transport' is '8' the value of this attribute must be '80'.



	R3013
	'ACTIVE BORDER TRANSPORT MEANS/Countries of routing of means of transport' first country in the sequence must be the same as 'CONSIGNMENT (MASTER LEVEL)/PLACE OF LOADING/UNLOCODE' or 'CONSIGNMENT (MASTER LEVEL)/PLACE OF LOADING/ADDRESS/Country'.



	R3014
	'ACTIVE BORDER TRANSPORT MEANS/Countries of routing of means of transport' last country in the sequence must be the same as 'CONSIGNMENT (MASTER LEVEL)/PLACE OF UNLOADING/UNLOCODE' or 'CONSIGNMENT (MASTER LEVEL)/PLACE OF UNLOADING/ADDRESS/Country'.



	R3016
	Each ‘Goods Item Number’ must be unique throughout CONSIGNMENT (MASTER LEVEL). The items shall be numbered in a sequential fashion, starting from '1' for the first item and incrementing the numbering by '1' for each following item.



	R3017
	Each ‘Goods Item Number’ must be unique throughout CONSIGNMENT (HOUSE LEVEL). The items shall be numbered in a sequential fashion, starting from '1' for the first item and incrementing the numbering by '1' for each following item.



	R3018
	The country of the COFE must be listed in the sequence of 'ACTIVE BORDER TRANSPORT MEANS/Countries of routing of means of transport'. 
In case the COFE begins with "XI" then "GB" must be listed in the 'ACTIVE BORDER TRANSPORT MEANS/Countries of routing of means of transport'.



	R3020
	The format of this attribute is 9999999-9.

	
R3021
	
The format of this attribute is ZZZZ9999999 (ISO 6346).



	R3022
	'COUNTRIES OF ROUTING OF CONSIGNMENT' must contain countries of 'PLACE OF ACCEPTANCE' and 'PLACE OF DELIVERY'.



	R3024
	This class/attribute cannot be amended.



	R3025
	Either 'DO NOT LOAD DETAILS/Receptacle identification numbers' or 'DO NOT LOAD DETAILS/TRANSPORT DOCUMENT (HOUSE LEVEL)' or 'DO NOT LOAD DETAILS/TRANSPORT EQUIPMENT' must be used.



	R3026
	When ADDITIONAL INFORMATION RESPONSE/BINARY ATTACHMENT/hashCode is used ADDITIONAL INFORMATION RESPONSE/BINARY ATTACHMENT/hashCodeAlgorithmnID must be used.



	R3028
	Either 'MRN', 'TRANSPORT DOCUMENT' or 'RECEPTACLE' must be used.



	R3029
	Either 'EXAMINATION PLACE/Place of examination' or 'EXAMINATION PLACE/Reference number' must be used.



	R3030
	At least one of the classes 'RECEPTACLE', 'GOODS ITEM', 'CONSIGNMENT (HOUSE LEVEL)', 'PACKAGING', 'TRANSPORT DOCUMENT', 'TRANSPORT EQUIPMENT' must be used.




	R3032
	Either 'CARRIER/Identification number' or 'CARRIER/Name' and 'CARRIER/ADDRESS' must be used.



	R3033
	'REPRESENTATIVE/Identification number' cannot be the same as 'DECLARANT/Identification number'.



	R3034
	Either the ‘CUSTOMS OFFICE OF FIRST ENTRY’ or ‘ADDRESSED MEMBER STATE’ is to be provided. 



	R3035
	Either the ‘Estimated date and time of departure’ or ‘Actual date and time of departure’ is to be provided. 


	R3046
	This message can contain 'ENS QUERY PARAMETERS' class only with one of the values in the attribute 'ENS QUERY PARAMETERS/Parameter' per combination:
Combination 1: ENSS or ENSH
Combination 2: ENSC or ENSF or ENSP

	
	

	R3048
	If the ‘RELATED TRANSPORT DOCUMENT’ is used, then the ‘RELATED MRN’ cannot be used.

	
	

	R3050
	This data is expected only when the message is provided by an Involved Member State.

	
	

	R3051
	Only value “2 – Sub-house level filing” can be used.

	R3052
	Each ‘Transport document (House level)’ must be unique throughout the ENS filing.

	R3053
	The 'Estimated date and time of arrival' cannot be earlier than the 'Actual date and time of departure' or 'Estimated date and time of departure'.


	R3055
	Either “Transport document (Master level)” or “Transport document (House level)” to be provided.



	R3056
	When 'ACTIVE BORDER TRANSPORT MEANS/Mode of transport' is '1' or '8', 
one of the following identifications has to be provided – 'Related MRN' or 'ACTIVE BORDER TRANSPORT MEANS/Identification number' and 'ACTIVE BORDER TRANSPORT MEANS/Frozen estimated date and time of arrival' or 'Related transport document' and 'ACTIVE BORDER TRANSPORT MEANS/Frozen estimated date and time of arrival'. 
When 'ACTIVE BORDER TRANSPORT MEANS/Mode of transport' is '3', one of the following identifications has to be provided – 'Related MRN' or 'ACTIVE BORDER TRANSPORT MEANS/Identification number' and 'ACTIVE BORDER TRANSPORT MEANS/Estimated date and time of arrival' or 'Related transport document' and 'ACTIVE BORDER TRANSPORT MEANS/Estimated date and time of arrival'.
When 'ACTIVE BORDER TRANSPORT MEANS/Mode of transport' is '2' or '4', one of the following identifications has to be provided – 'Related MRN' or 'ACTIVE BORDER TRANSPORT MEANS/Conveyance reference number' and 'ACTIVE BORDER TRANSPORT MEANS/Estimated date and time of arrival' or 'Related transport document' and 'ACTIVE BORDER TRANSPORT MEANS/Estimated date and time of arrival'.
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	C3001
	IF 'SPLIT CONSIGNMENT/Split consignment indicator' is set to '1', 
THEN this data attribute is M, 
ELSE it is not used.



	C3003
	IF 'CONSIGNMENT (MASTER LEVEL)/PLACE OF ACCEPTANCE/UNLOCODE' is not provided, 
THEN this attribute/class is M, 
ELSE it is not used.



	C3004
	IF 'CONSIGNMENT (HOUSE LEVEL)/PLACE OF ACCEPTANCE/UNLOCODE' is not provided, 
THEN this attribute/class is M, 
ELSE it is not used.



	C3005
	IF 'CONSIGNMENT (MASTER LEVEL)/PLACE OF DELIVERY/UNLOCODE' is not provided, 
THEN this attribute/class is M, 
ELSE it is not used.



	C3006
	IF 'CONSIGNMENT (HOUSE LEVEL)/PLACE OF DELIVERY/UNLOCODE' is not provided, 
THEN this attribute/class is M, 
ELSE it is not used.



	C3007
	IF 'CONSIGNMENT (MASTER LEVEL)/PLACE OF LOADING/UNLOCODE' is not provided, 
THEN this attribute/class is M, 
ELSE it is not used.



	C3008
	IF 'CONSIGNMENT (MASTER LEVEL)/PLACE OF UNLOADING/UNLOCODE' is not provided,
THEN this attribute/class is M, 
ELSE it is not used.



	C3009
	IF 'RISK ANALYSIS RESULT/Risk analysis type' is set to 'E', 'G', 'S' or 'X', and 'RISK ANALYSIS RESULT/Result code' is set to '1', '2', '3, '5' or '6',
THEN 'RISK ANALYSIS RESULT/Risk criteria' is M, 
ELSE it is O.



	C3010
	IF 'RISK ANALYSIS RESULT/Risk analysis type' is set to 'Z', 
THEN 'RISK ANALYSIS RESULT/Result code' is O, 
ELSE it is M.



	C3011
	IF 'RISK ANALYSIS RESULT/Risk analysis type' is set to 'Z' or 'RISK ANALYSIS RESULT/Result code' is set to '2-Risk downgraded – no further action necessary', '3-Risk not confirmed – false positive' or '4-No risk' , 
THEN this class is O, 
ELSE it is M.



	C3012
	IF 'ACTIVE BORDER TRANSPORT MEANS/Mode of transport' is set to '1', '3' or '8', 
THEN this data attribute is M, 
ELSE it is not used.



	C3013
	IF 'CONSIGNMENT (MASTER LEVEL)/Container indicator' is set to '1', 
THEN this class is M at 'CONSIGNMENT (MASTER LEVEL)' or 'CONSIGNMENT (MASTER LEVEL)/GOODS ITEM', 
ELSE it is not used.



	C3014
	IF 'CONSIGNMENT (HOUSE LEVEL)/Container indicator' is set to '1', 
THEN this class is M at 'CONSIGNMENT (HOUSE LEVEL)' or 'CONSIGNMENT (HOUSE LEVEL)/GOODS ITEM', 
ELSE it is not used.



	C3015
	IF 'CONSIGNMENT (MASTER LEVEL)/TRANSPORT EQUIPMENT/Number of seals' is used, 
THEN this classis M, 
ELSE it is not used.



	C3016
	IF 'CONSIGNMENT (MASTER LEVEL)/GOODS ITEM/TRANSPORT EQUIPMENT/Number of seals' is used,
THEN this classis M, 
ELSE it is not used.



	C3017
	IF 'CONSIGNMENT (HOUSE LEVEL)/TRANSPORT EQUIPMENT/Number of seals' is used, 
THEN this classis M, ELSE it is not used.

	
C3018
	
IF 'CONSIGNMENT (HOUSE LEVEL)/GOODS ITEM/TRANSPORT EQUIPMENT/Number of seals' is used,
THEN this classis M, 
ELSE it is not used.



	C3019
	IF 'ACTIVE BORDER TRANSPORT MEANS/Mode of transport' is set to '2' or '4', 
THEN this data attribute is M, 
ELSE it is not used.



	C3020
	IF 'CONSIGNMENT (HOUSE LEVEL)/PLACE OF DELIVERY/UNLOCODE' 2 first characters or 'CONSIGNMENT (HOUSE LEVEL)/PLACE OF DELIVERY/ADDRESS/Country' refers to EU MS, 
THEN this class is M, 
ELSE it is O.



	C3022
	IF 'CONSIGNMENT (HOUSE LEVEL)/ADDITIONAL INFORMATION/Code' is '10600', 
THEN this class is O, 
ELSE it is M.



	C3024
	IF 'CONSIGNMENT (HOUSE LEVEL)/ADDITIONAL INFORMATION/Code' is '10600', 
THEN this class is M, 
ELSE it is O.



	C3025
	IF 'CONSIGNMENT (HOUSE LEVEL)/CONSIGNOR/Type of person' and 'CONSIGNMENT (HOUSE LEVEL)/CONSIGNEE/Type of person' is '1 (Natural person)', 
THEN attribute is O, 
ELSE it is M.



	C3034
	IF 'ADDRESS/Country' in CL733 has a country code with postal code indicator 'C', 
THEN this attribute in the same class is O, 
ELSE it is M.



	C3035
	IF 'CONSGINMENT (MASTER LEVEL)/GOODS ITEM/PACKAGING/Type of packages' is 'VQ', 'VG', 'VL', 'VY', 'VR', 'VS', 'VO', 'NE', 'NF', 'NG', 
THEN this attribute is not used, 
ELSE it is M.



	C3036
	IF 'CONSGINMENT (HOUSE LEVEL)/GOODS ITEM/PACKAGING/Type of packages' is 'VQ', 'VG', 'VL', 'VY', 'VR', 'VS', 'VO', 'NE', 'NF', 'NG', 
THEN this attribute is not used, 
ELSE it is M.



	C3037
	IF 'CONSIGNMENT (HOUSE LEVEL)/ADDITIONAL INFORMATION/Code' contains value
‘10900’ and 'CONSIGNMENT (HOUSE LEVEL)/ADDITIONAL FISCAL REFERENCES' class is not provided
THEN this class/attribute is M, 
ELSE it is O.



	C3038
	IF 'CONSIGNMENT (HOUSE LEVEL)/ADDITIONAL INFORMATION/Code' contains value ‘10900’ 
THEN this class/attribute is M, 
ELSE it is O.

	
	

	C3039
	IF ‘CONTROL DECISION/Control decision’ is set to ‘0 (No control)’, 
THEN this attribute is M, 
ELSE it is O.

	
	

	C3040
	IF ‘CONTROL DECISION/Control decision’ is set to ‘1 (Control)’, 
THEN this attribute is M, 
ELSE it is not to be used.

	
	

	
	

	C3043
	IF ‘RISK ANALYSIS/Category’ is set to ‘F’ and ‘RISK ANALYSIS RESULT/Result code’ is set to ‘1’ and ‘DO NOT LOAD DETAILS’ class is not used,
THEN this class is M,
ELSE this class is O.


	C3044
	IF in the same 'RISK ANALYSIS' class the combination of ‘RISK ANALYSIS/Category’ set to ‘A’, ‘RISK ANALYSIS RESULT/Risk analysis type’ set to ‘X’ and ‘RISK ANALYSIS RESULT/Result code’ set to ‘1’ appears at least once
THEN this class is M,
ELSE
IF in the same 'RISK ANALYSIS' class the combination of ‘RISK ANALYSIS/Category’ set to ‘F’, ‘RISK ANALYSIS RESULT/Risk analysis type’ set to ‘S’ and ‘RISK ANALYSIS RESULT/Result code’ set to ‘1’ appears at least once
THEN this class is O,
ELSE it cannot be used.


	C3045
	IF ’Requested ENS data’ is set to ‘1-True’ or class ‘TRANSPORT EQUIPMENT’ is used, 
THEN this attribute is M,
ELSE this attribute is O.

	
	

	C3046

	IF ‘TRANSPORT DOCUMENT (HOUSE LEVEL)/Type’ is ‘703 - House air waybill’ or ‘740 - Airway bill’ (general)’,
THEN this class is M,
 ELSE this class is O.


	C3047
	If the 'Risk analysis result/Result code' is '6' or '7', 
THEN this classis 'M', 
ELSE this class is 'O'.

	
	

	C3048
	IF 'CONSIGNMENT (MASTER LEVEL)/CONSIGNOR/Type of person' and 'CONSIGNMENT (MASTER LEVEL)/CONSIGNEE/Type of person' is '1 (Natural person)', 
THEN attribute is O, 
ELSE it is M.

	
	

	C3049
	If the Arrival notification is provided via a National Arrival System (not via the STI), then the ‘PERSON NOTIFYING THE ARRIVAL’ is O, else it is M.

	
	

	C3050
	IF 'CONSIGNMENT (MASTER LEVEL)/Container indicator' is set to '1', 
THEN this class is M, 
ELSE it is not used.

	
	

	C3051
	IF 'CONSIGNMENT (HOUSE LEVEL)/Container indicator' is set to '1', 
THEN this class is M, 
ELSE it is not used.

	
	

	C3052
	IF the combination of ‘RISK ANALYSIS RESULT/Risk analysis type’ set to ‘E’ and ‘RISK ANALYSIS RESULT/Result code’ set to ‘5’ appears at least once for ‘RISK ANALYSIS/Category’ ‘A’
THEN this class is M,
ELSE
IF the combination of ‘RISK ANALYSIS RESULT/Risk analysis type’ set to ‘G’ and ‘RISK ANALYSIS RESULT/Result code’ set to ‘5’ appears at least once for ‘RISK ANALYSIS/Category’ ‘F’
THEN this class is O,
ELSE it cannot be used.

	C3053
	This attribute is M when it is provided by SSA, otherwise it is not used.

	C3054
	IF the ‘Request pre-loading risk assessment status/Consignment (House level)/Status/Code’ is set to ‘RFI’, ‘RFS’ or ‘AMD’
THEN this data attribute is M, 
ELSE it is not used.

	C3055
	IF the ‘Request pre-loading risk assessment status’ is set to ‘1’
THEN a list of receptacles OR an ENS MRN OR a Transport document (Master level) is M.

	C3056
	IF the ‘Active border transport means/Mode of transport’ is set to ‘2’
THEN the ‘Active border transport means/Nationality’ it is not used
ELSE it is M.
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